../Core/Src/ad5934_driver.c:47:6:AD5934_SetRegisterValue	2
../Core/Src/ad5934_driver.c:75:10:AD5934_GetRegisterValue	3
../Core/Src/ad5934_driver.c:114:10:AD5934_ReadRegister	3
../Core/Src/ad5934_driver.c:151:6:AD5934_Init	1
../Core/Src/ad5934_driver.c:182:6:AD5934_RestartSweep	1
../Core/Src/ad5934_driver.c:214:6:AD5934_Repeat_Sweep	1
../Core/Src/ad5934_driver.c:227:6:AD5934_StopSweep	1
../Core/Src/ad5934_driver.c:244:10:AD5934_Sweep	1
../Core/Src/ad5934_driver.c:270:7:AD5934_Get_Ref_Resistance	4
../Core/Src/ad5934_driver.c:321:7:AD5934_GetTemperature	5
../Core/Src/ad5934_driver.c:411:7:AD5934_Calculate_Temperature	3
../Core/Src/ad5934_driver.c:452:7:AD5934_GetImpedance	10
../Core/Src/ad5934_driver.c:528:7:AD5934_GetMagnitude	1
../Core/Src/ad5934_driver.c:549:6:AD5934_Wait_For_Data_Valid	3
../Core/Src/ad5934_driver.c:584:10:AD5934_Compress_To_IntScale	5
../Core/Src/ad5934_driver.c:614:7:AD5934_Round_Float_Precision	2
../Core/Src/ad5934_driver.c:639:7:AD5934_Linear_Correction	1
../Core/Src/ad5934_driver.c:656:7:AD5934_EC_Compensate_To_25C	2
../Core/Src/ad5934_driver.c:672:7:AD5934_EC_Calibrate_Temperature	5
../Core/Src/ad5934_driver.c:721:7:AD5934_Calibrate	1
../Core/Src/ad5934_driver.c:737:6:AD5934_Process_System	24
../Core/Src/ad5934_driver.c:862:6:AD5934_Sort_Array	4
../Core/Src/ad5934_driver.c:884:7:AD5934_Trimmed_Mean	3
../Core/Src/ad5934_driver.c:910:7:AD5934_History_Average	2
../Core/Src/ad5934_driver.c:924:6:AD5934_Process_Sample	4
../Core/Src/ad5934_driver.c:970:6:AD5934_RTD_NewSample	1
../Core/Src/ad5934_driver.c:977:6:AD5934_EC_NewSample	1
../Core/Src/ad5934_driver.c:984:6:AD5934_Reference_NewSample	1
../Core/Src/ad5934_driver.c:1000:6:ADG715_SetRegisterValue	1
../Core/Src/ad5934_driver.c:1010:6:ADG715_SetChannels	1
../Core/Src/ad5934_driver.c:1015:6:ADG715_ResetChannels	1
../Core/Src/ad5934_driver.c:1027:6:ADG715_Update	2
