../Core/Src/ad5934_driver.c:33:6:AD5934_SetRegisterValue	32	static
../Core/Src/ad5934_driver.c:61:10:AD5934_GetRegisterValue	40	static
../Core/Src/ad5934_driver.c:100:10:AD5934_ReadRegister	48	static
../Core/Src/ad5934_driver.c:137:6:AD5934_Init	8	static
../Core/Src/ad5934_driver.c:165:6:AD5934_RestartSweep	8	static
../Core/Src/ad5934_driver.c:195:10:AD5934_Sweep	16	static
../Core/Src/ad5934_driver.c:221:7:AD5934_Get_Ref_Resistance	48	static
../Core/Src/ad5934_driver.c:272:7:AD5934_GetTemperature	72	static
../Core/Src/ad5934_driver.c:360:7:AD5934_GetImpedance	56	static
../Core/Src/ad5934_driver.c:431:6:AD5934_Wait_For_Data_Valid	24	static
../Core/Src/ad5934_driver.c:466:7:AD5934_Round_Float_Precision	24	static
../Core/Src/ad5934_driver.c:491:7:AD5934_Linear_Correction	24	static
../Core/Src/ad5934_driver.c:508:7:AD5934_EC_Compensate_To_25C	24	static
../Core/Src/ad5934_driver.c:524:7:AD5934_EC_Calibrate_Temperature	152	static
../Core/Src/ad5934_driver.c:573:7:AD5934_Calibrate	48	static
../Core/Src/ad5934_driver.c:598:6:ADG715_SetRegisterValue	32	static
../Core/Src/ad5934_driver.c:608:6:ADG715_SetChannels	16	static
../Core/Src/ad5934_driver.c:613:6:ADG715_ResetChannels	8	static
../Core/Src/ad5934_driver.c:625:6:ADG715_Update	16	static
